


**DS-2CD1123G0-I**

**2.0 MP IR Network Dome Camera**

|  |  |
| --- | --- |
| E:\Working Folder\work\work\201610\1系列的spec, 10月为2系列的spec\海外低端1系列(无Hiwatch series丝印版)\HIW1系列NO LOGO\DS-2CD1101-I'DS-2CD1121-I .jpg | E:\Working Folder\work\work\201610\1系列的spec, 10月为2系列的spec\效果图\11xx 2圈灯.jpg |
| 2.8 mm Fixed Lens | Non 2.8 mm Fixed Lens |
|  |  |

|  |  |
| --- | --- |
| **Key Features** | |
| * 1/2.8" progressive scan CMOS | * 3D DNR (Digital Noise Reduction) |
| * 1920 × 1080@30fps | * Up to 30 m IR range |
| * 2.8 mm/4 mm/6 mm fixed lens | * PoE (Power over Ethernet) |
| * H.265+, H.265, H.264+, H.264 | * IP67, IK10 |
| * Dual stream |  |
| * Digital WDR (Wide Dynamic Range) |  |

|  |  |
| --- | --- |
| ***Camera***  **Specification** | |
| Image Sensor | 1/2.8" progressive scan CMOS |
| Min. Illumination | Color: 0.01 Lux @(F1.2, AGC ON), 0.028Lux @ (F2.0, AGC ON) |
| Shutter Speed | 1/3 s to 1/100, 000 s |
| Slow Shutter | Yes |
| Auto-Iris | No |
| Day &Night | IR cut filter |
| Digital Noise Reduction | 3D DNR |
| WDR | Digital WDR |
| Angle Adjustment | Pan: 0° to 355°, tilt: 0° to 70° |
| ***Lens*** | |
| Focal length | 2.8 mm, 4 mm, 6 mm |
| Aperture | F2.0 |
| Focus | No |
| FOV | 2.8 [mm,](mailto:mm@F2.0) horizontal FOV 114°, vertical FOV 62°, diagonal FOV 135°  4 mm, horizontal FOV 86°, vertical FOV 46°, diagonal FOV 102°  6 mm, horizontal FOV 54°, vertical FOV 30°, diagonal FOV 62° |
| Lens Mount | M12 |
| ***IR*** | |
| IR Range | Up to 30 m |
| Wavelength | 850 nm |
| ***Compression Standard*** |  |
| Video Compression | Main stream: H.265/H.264  Sub stream: H.265/H.264/MJPEG |
| H.264 Type | Baseline Profile/Main Profile/High Profile |
| H.264+ | Main stream supports |
| H.265 Type | Main Profile |
| H.265+ | Main stream supports |
| Video Bit Rate | 32 Kbps to 8 Mbps |
| ***Smart Feature-set*** | |
| Region of Interest | 1 fixed region for main stream and sub-stream |
| ***Image*** | |
| Max. Resolution | 1920 × 1080 |
| Main Stream  Max. Frame Rate | 50Hz: 25fps (1920 × 1080, 1280 × 960, 1280 × 720)  60Hz: 30fps (1920 × 1080, 1280 × 960, 1280 × 720) |
| Sub-stream  Max. Frame Rate | 50Hz: 25fps (640 × 480, 640 × 360, 320 × 240)  60Hz: 30fps (640 × 480, 640 × 360, 320 × 240) |
| Image Enhancement | BLC, 3D DNR |
| Image Setting | Saturation, brightness, contrast, sharpness, AGC, white balance adjustable by client software or web browser |
| Day/Night Switch | Auto, scheduled |
| ***Network*** | |
| Alarm Trigger | Motion detection, video tampering alarm, illegal login |
| Protocols | TCP/IP, ICMP, HTTP, HTTPS, FTP, DHCP, DNS, DDNS, RTP, RTSP, RTCP, NTP, UPnP, SMTP, IGMP, 802.1X, QoS, IPv6, UDP, Bonjour |
| General Function | Anti-flicker, heartbeat, mirror, password protection, privacy mask, watermark |
| Firmware Version | 5.5.2 |
| API | ONVIF (PROFILE S, PROFILE G), ISAPI |
| Simultaneous Live View | Up to 6 channels |
| User/Host | Up to 32 users  3 levels: Administrator, Operator, and User |
| Client | iVMS-4200, Hik-Connect, iVMS-5200 |
| Web Browser | IIE7+, Chrome18-42, Firefox5.0+, Safari5.02+ |
| ***Interface*** |  |
| Communication Interface | 1 RJ45 10M/100M self-adaptive Ethernet port |
| ***General*** | |
| Operating Conditions | -30 °C to 50 °C (-22 °F to 122 °F), humidity: 95% or less (non-condensing) |
| Power Supply | 12 VDC ± 25%, 5.5 mm coaxial power plug  PoE (802.3af, class 3) |
| Power Consumption and Current | 12 VDC, 0.4 A, Max: 5 W  PoE: (802.3af, 37 V to 57 V), 0.2 A to 0.13 A, Max: 7 W |
| Ingress Protection | IP67, IK10  TVS 2000V lightning protection, surge protection and voltage transient protection |
| Material | Metal & Plastic |
| Dimensions | Camera: Ø 111 mm × 82.4 mm ( 4.4" × 3.2")  With package: 134 mm × 134 mm × 108 mm (5.3" × 5.3" × 4.3") |
| Weight | Camera: Approx. 410 g (0.9 lb.)  With package: Approx. 610 g (1.3 lb.) |

|  |
| --- |
| **Available Models** |
| DS-2CD1123G0-I (2.8 mm), DS-2CD1123G0-I (4 mm), DS-2CD1123G0-I (6 mm) |

|  |
| --- |
| **Dimension** |



|  |  |  |  |
| --- | --- | --- | --- |
| **Accessory** | | | |
| 未标题-2.png  DS-1259ZJ  Inclined Base Mounting Bracket | DS-1275ZJ-SUS  Vertical Pole Mount | E:\Working Folder\work\work\去掉背景的支架\DS-1273ZJ-135.png  DS-1273ZJ-135  Wall Mount | E:\Working Folder\work\work\去掉背景的支架\DS-1273ZJ-135B.png  DS-1273ZJ-135B  Wall Mount |
| DS-1271ZJ-135  Pendant Mount | DS-1276ZJ-SUS  Corner Mount | E:\Working Folder\work\work\去掉背景的支架\DS-1280ZJ-DM21.png  DS-1280ZJ-DM21  Junction Box | DS-1250ZJ  Rain Shade |

050520180120

050520170918

050440161122